3D HOLOGRAM

Procedure:

4 sheets of acrylic were used for the making of this hologram, the 4 sheets were cut in particular shape and connected with each other such that on one end a square shape was formed. the size of the square was equal to that of the screen. Complete darkness is to be maintained during this.

The 3D hologram works on the principle of reflection and it makes an image which is going on the screen. A reference video link is added below for reference

<https://youtu.be/7YWTtCsvgvg>

The above video was used as reference and the measurements were increased as required. A logo was used to display through this hologram.